“Análisis de Nodos”

Practice 7

Cabañas Baxcajay Jesús Francisco

Hernández Velázquez Ángel

Martínez Coronel Brayan Yosafat

1CM10

May 20th, 2019

Index

[Practice development 2](#_Toc9282137)

[Questionary 3](#_Toc9282138)

[What is a node in an electric circuit? 3](#_Toc9282139)

[What is voltage node? 3](#_Toc9282140)

[what is a reference node? 3](#_Toc9282141)

[Describe how to use node analysis 3](#_Toc9282142)

[Demonstrate that an reactive element has zero watts of electric power 3](#_Toc9282143)

[Conclusions 3](#_Toc9282144)

[Cabañas Baxcajay Jesús Francisco 3](#_Toc9282145)

[Hernández Velázquez Ángel 4](#_Toc9282146)

[Martínez Coronel Brayan Yosafat 4](#_Toc9282147)

[Calculations 4](#_Toc9282148)

[Simulations 4](#_Toc9282149)

# Practice development

Using node analysis method with the circuit below. Built the circuit and measure the values required in the table 1.

Imagen que contiene texto

Descripción generada automáticamente

Table of Values 1

|  |  |
| --- | --- |
| Points | Measured Values (amps) |
| II,0 | 407 micro |
| III,I | 2.85 milli |
| III,0 | 26.6 milli |

Now, get voltage values and fill the table below.

Table of Values 2

|  |  |
| --- | --- |
| Points | Measured Values (volts) |
| VI,0 | 438.57 milli |
| VII,I | 3.1912 |
| VII,0 | 3.05 |

Finally, get power values and fill the table below.

Table of Values 3

|  |  |
| --- | --- |
| Resistor | Power (watts) |
| R1 | 1.65x10-4 |
| R2 | 8.12x10-3 |
| R3 | 0.707 |

# Questionary

## What is a node in an electric circuit?

A node is a place where two or more components have a common connection.

## What is voltage node?

By Electric Current Kirchhoff Law, we know no charge can be accumulated in any node.

## what is a reference node?

The most used node (which connects most of the elements).

## Describe how to use node analysis

Identify node ubications.

Select a reference node and connect it with ground.

Assign a voltage value on every node.

Assign electric current directions.

Get the equations.

Resolve those equations.

## Demonstrate that an reactive element has zero watts of electric power

We know that Power is equal to V x I x cosβ/2, but voltage and electric current always have ±90 degrees, and cos of 90 degrees is 0, no matters what inductor or capacitor you put, the angle is the same, so (number of voltage) x (number of electric current) x (zero)/2, is always zero.

# Conclusions

## Cabañas Baxcajay Jesús Francisco

The node analysis in circuits is a very useful method where we locate points where two or more elements cross. We must find an equation for each node, using Kirchhoff Law. We observed that node analysis is possible when all nodes have conductance. This method is practical, simple and sometimes it reduces time. It's important that we observed carefully the circuit to choose the best method to solve it.

## Hernández Velázquez Ángel

The analysis of a circuit by the method of nodes helps us obtain equations to calculate the current, voltage or value of certain components so that the necessary is fulfilled. This method must be used with care because in many cases it can become a double-edged sword that damages the calculation instead of facilitating it.

## Martínez Coronel Brayan Yosafat

Node analysis (like other techniques) make a faster work, so the productivity of every of us is increased by this. That is amazing, because if we can do the same things than before, but faster, it means we can resolve more problems in less time. If we make it perfect, we can just resolve every circuit.

# Calculations

There were no calculations.

# Simulations




Imagen que contiene texto

Descripción generada automáticamente